|  |  |  |
| --- | --- | --- |
| **REQUEST FOR QUOTATION (RFQ)** | | Supplier’s Stamp/Signature: |
| Closing Date | : **12** **June 2025** |
| Email Submission | : **box4@belts.com.bn** |
| BELTS Ref | : **BELTS/HCCS/RFQ/2025/015** |
| Date of Submission | : Click here to enter text. |
| Supplier/Quote Ref | : Click here to enter text. |

|  |  |
| --- | --- |
| Company Name | **Click here to enter text.** |
| Address | **Click here to enter text.** |
| Phone | Office: **Click here to enter text.** Mobile: **Click here to enter text.** |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **No.** | **Item Description** | **Delivery Period** | **Qty/UoM** | **Unit Price** | **Total Price** |
| **1** | **1 YEAR QUARTERLY PREVENTIVE MAINTENANCE OF PHARMACEUTICAL FREEZERS**  Preventive maintenance period:  Frequency: **Quarterly.**  Period: **1st September 2025 until 31st August 2026.**  Location**:**  **Medical Supply Chain (MSC) Simpang 433, Rimba Highway, Kampong Madaras.**  Quantity:   1. **UL-FREEZERS** (3 units of Haier Biomedical brand & 1 unit of China brand). 2. **DEEP FREEZERS** (4 units of Haier Biomedical brand). 3. **FREEZER** (1 unit of US CHEF brand). | **01 SEPTEMBER 2025 UNTIL 31 AUGUST 2026** | **4 AU** | **Click here to enter text.** | **Click here to enter text.** |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **No.** | **Item Description** | **Delivery Period** | **Qty/UoM** | **Unit Price** | **Total Price** |
|  | Scope of work for PHARMACEUTICAL FREEZERS**:**   * General servicing * Clean the condenser coil and filter * Temperature verification/validation * Clean the door gaskets and scape gasket * Removal of frost and ice buildup * Check the refrigerant charging and leakage * Check and validation of power supply, compressor performance, condensing fan motor * Replacement of back-up battery **(if needed only)** * Defrost the chamber **(if needed only)** * Monitor the vacuum relief port **(once per use, if applicable)** * Check UPS performance (if available) * UPS Battery to be quoted separately if it is required for replacement.   **Remarks:**   1. To attach preventive maintenance chart individually at the unit itself. 2. Preventive maintenance shall include at minimum, but not limited to, checking all components of freezer units, including the condenser, evaporator and controller. 3. Preventive maintenance services should take place during normal business working hours (Monday to Thursday and Saturday, from 0800 until 1630). 4. For emergency call, troubleshooting and repair, to quote separately upon approval. 5. To quote separately on any defective/faulty parts, consumables, controller, refrigerant etc. |  |  |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **No.** | **Item Description** | **Delivery Period** | **Qty/UoM** | **Unit Price** | **Total Price** |
| **2** | **1 YEAR QUARTERLY PREVENTIVE MAINTENANCE OF PHARMACEUTICAL REFRIGERATORS**  Preventive maintenance period:  Frequency: **Quarterly.**  Period: **1st September 2025 until 31st August 2026.**  Location**:**  **Medical Supply Chain (MSC) Simpang 433, Rimba Highway, Kampong Madaras.**  Quantity:  **2 units.**  Scope of work for PHARMACEUTICAL REFRIGERATOR:   * Visually inspect units for sign of corrosion of fins, cabinet, copper tubing and solder joints. * Inspect for excessive or unusual vibration for fan blades or sheet metal panels when in operation. * Identify fan cells causing vibration and check motor and blade carefully. * Check for stains, return bends and coil fins, drain pans. * Clean the evaporator coils and blades * Flush and rinse coil for any traps/blockage. * Check each fan for quiet, free and proper rotation. * Check screws and tighten as necessary. * Oil motors as required. * Check all electrical wiring and components, check the heaters to ensure even surface contact with the coil. * Check the drain line heat tape for proper operation, look for abnormal accumulation of ice patterns, and adjust defrost cycles accordingly. * Check refrigerant cycle, unit cooler superheat and compare readings. * Visually check condensing units for moisture conditions, check the sight glass for proper oil levels, inspect wiring, check for debris and dirt, and unusual vibration or noises. * Check operation of all timers, relays, pressure controls and safety controls, filters and driers. * Validation/Calibration certificate per unit, sticker with validity. | **01 SEPTEMBER 2025 UNTIL 31 AUGUST 2026** | **4 AU** | **Click here to enter text.** | **Click here to enter text.** |

|  |  |  |  |
| --- | --- | --- | --- |
|  | Remarks:   1. To attach preventive maintenance chart individually at the unit itself. 2. Preventive maintenance shall include at minimum, but not limited to, checking all components of freezer units, including the condenser, evaporator and controller. 3. Preventive maintenance services should take place during normal business working hours (Monday to Thursday and Saturday, from 0800 until 1630) 4. For emergency call, troubleshooting and repair, to quote separately upon approval. 5. To quote separately on any defective/faulty parts, consumables, compressor, motor, controller, refrigerant etc. | | |
| **MANDATORY**  Suppliers are to provide with the Packaging Dimension, Measurement & Weight - in Standard measurement in Meter, Feet, Inches, Cm, Mm, Kg, GM | | **TOTAL PRICE** | **Click here to enter text.** |
| Freight Term (EXW,CIF,ETC) | | | **Click here to enter text.** |
| Freight Charges (IF APPLICABLE) | | | **Click here to enter text.** |
| Any other charges please state | | | **Click here to enter text.** |
| **GRAND TOTAL** | | | **Click here to enter text.** |

|  |  |
| --- | --- |
| Currency Code : | **BND** |
| Price Validity  (Minimum 9 Months) : | **Click here to enter text.** |
| Payment Terms : | **30 DAYS CREDIT** |
| Warranty : | **Click here to enter text.** |
| Mode of Delivery : | **Click here to enter text.** |
| Delivery Period : | **Click here to enter text.** |
| Country of Manufactured : | **Click here to enter text.** |
| Remarks: | **Click here to enter text.** |