|  |  |  |
| --- | --- | --- |
| **REQUEST FOR QUOTATION (RFQ)** | | Supplier’s Stamp/Signature: |
| Closing Date | : **8** **September 2025** |
| Email Submission | : **box6@belts.com.bn** |
| BELTS Ref | : **BELTS/HCCS/RFQ/2025/023** |
| Date of Submission | : Click here to enter text. |
| Supplier/Quote Ref | : Click here to enter text. |

|  |  |
| --- | --- |
| Company Name | **Click here to enter text.** |
| Address | **Click here to enter text.** |
| Phone | Office: **Click here to enter text.** Mobile: **Click here to enter text.** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **No.** | **Item Description** | **Delivery Period** | **Qty/UoM** | | **Unit Price** | | **Total Price** |
| ANTI MOULD TREATMENT AND COATING WORKS TO EXTERNAL AND INTERNAL FACES OF THE AFFECTED WALLS AT THE ENTRANCE MAIN HALLWAY NEAR TO MALE SURAU ROOM, GROUND FLOOR AT BELTS MEDICAL SUPPLY CHAIN (MSC). | | | | | | | |
| **1** | **SCOPE OF WORK:**  **a. Mobilisation and scaffolding works.**   * To deliver the scaffolding and erect at site where ever required for this project to access for application of the treatment, cleaning works and coating works. | **2-3 WORKING DAYS UPON PO ISSUANCE & PTW APPROVAL** | **1 LOT** | | **Click here to enter text.** | | **Click here to enter text.** | |
| **b. Internal walls.**   * To do insulation works on the internal faces of the affected walls first by cleaning the surfaces. * Supply and install 3mm thick calcium silicate boards on 3” metal framing supports. * To do the final finishing by application of 1 coat **ISONEM Primer** and 2 coats of **ISONEM Thermal Paint.**   Measurement area:  Approx 110 m2 | **1 LOT** | | **Click here to enter text.** | | **Click here to enter text.** | |
| **c. Internal ceiling works.**   * To install scaffolding to access the ceiling. * To apply Greenex anti-mould treatment and allow to react for 3 days where required. * To apply Omniclean cleaning chemical and wash clean the treated ceiling areas. * To apply 1 coat of waterbased primer and 2 coats of emulsion paint to match the existing as close as possible.   Measurement area:  Approx 50m2 | **1 LOT** | | **Click here to enter text.** | | **Click here to enter text.** | |
| **2** | **a. External walls.**  Surface treatment and cleaning works.   * To spray apply the whole surface of the affected walls with anti mould chemical **WVT Greenex** and allow to react for 3 days. * To spray apply the cleaning chemical, **WVT Omniclean** and allow to react for at least 15 minutes and then to clean by high pressure water jetting.   Measurement area:  Approx 178m2 | **1 LOT** | | **Click here to enter text.** | | **Click here to enter text.** | |
| **b. Coating works.**   * To supply and apply 1 coat of **ISONEM Primer.** * To apply 2 coats of **ISONEM Thermal Paint** to the treated walls.   Measurement area:  Approx 178m2 | **1 LOT** | | **Click here to enter text.** | | **Click here to enter text.** | |
| **3** | **Greasing of roller shutters.**   * To provide labour, equipment and materials to clean and re-grease the affected motor operated roller shutters:  1. IV room shutter (near receiving area). 2. Receiving area main entrance shutter. 3. Receiving area to warehouse shutter. 4. Delivery area preparation room shutter. 5. Delivery area exit shutter. | **5 UN** | | **Click here to enter text.** | | **Click here to enter text.** | |
|  | **Note:**   * **The address is at:** * BELTS Medical Supply Chain (MSC), Spg 433, Rimba Highway, Kg. Madaras. * For any site visit request, kindly email your proposed date & time schedule to [admincorp@belts.com.bn](mailto:admincorp@belts.com.bn) * For any questions or enquiries kindly e-Mail directly to [rfq\_enquiry@belts.com.bn](mailto:rfq_enquiry@belts.com.bn) * Contractors must implement safety measures to protect workers and public during installation/delivery work. * Vendors/contractors must adhere to regulatory SHENA safety rules and regulations. * The vendor awarded for this RFQ must submit a complete Permit To Work (PTW) document checklists requested for the work. | | | | | | |
| **MANDATORY**  Suppliers are to provide with the Packaging Dimension, Measurement & Weight - in Standard measurement in Meter, Feet, Inches, Cm, Mm, Kg, GM | | | | **TOTAL PRICE** | | **Click here to enter text.** | |
| Freight Term (EXW,CIF,ETC) | | | | | | **Click here to enter text.** | |
| Freight Charges (IF APPLICABLE) | | | | | | **Click here to enter text.** | |
| Any other charges please state | | | | | | **Click here to enter text.** | |
| **GRAND TOTAL** | | | | | | **Click here to enter text.** | |

|  |  |
| --- | --- |
| Currency Code : | **BND** |
| Price Validity  (Minimum 9 Months) : | **Click here to enter text.** |
| Payment Terms : | **30 DAYS CREDIT** |
| Warranty : | **Click here to enter text.** |
| Mode of Delivery : | **Click here to enter text.** |
| Delivery Period : | **Click here to enter text.** |
| Country of Manufactured : | **Click here to enter text.** |
| Remarks: | **Click here to enter text.** |