|  |  |  |
| --- | --- | --- |
| **REQUEST FOR QUOTATION (RFQ)** | | Supplier’s Stamp/Signature: |
| Closing Date | **: 28 November 2025** |
| Email Submission | **: box5@belts.com.bn** |
| BELTS Ref | : **BELTS/LSS-FM/RFQ/2025/001** |
| Date of Submission | : Click here to enter text. |
| Supplier/Quote Ref | : Click here to enter text. |

|  |  |
| --- | --- |
| Company Name | **Click here to enter text.** |
| Address | **Click here to enter text.** |
| Phone | Office: **Click here to enter text.** Mobile: **Click here to enter text.** |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **No.** | **Item Description** | **Delivery Period** | **Qty/UoM** | | **Unit Price** | **Total Price** |
| The contractor shall carry out the replacement of defective lamps at BELTS Simulation Training Centre, Penanjong Camp. The objective of this work is to ensure all lighting fixtures within the facility are restored to proper working conditions, improving overall illumination and energy efficiency.  The scope of work shall include, but is not limited to, the following:   * Supply and install equivalent or approved LED lamps as specified below, ensuring compatibility with existing fittings and electrical systems. * Replace all defective lamps with new, energy-efficient LED units that meet approved technical specifications. * Proper disposal of old lamps in accordance with HSE requirements. * Testing and verification to ensure all replaced lamps are functioning properly. * Submit a completion report confirming the total number of lamps replaced, test results and any observations | | | | | | |
| **1.** | **Replacement of the following defective lamps:** | | | | | |
| **A** | **Location: SAT 1** |  | | | | |
|  | * Type: 18W LED tube (daylight) |  | **2** | | **Click here to enter text.** | **Click here to enter text.** |
| * Type: 36W Fluorescent tube (daylight) |  | **1** | | **Click here to enter text.** | **Click here to enter text.** |
| * Type: Dimmable ballast for 2x36W fluorescent fitting |  | **1** | | **Click here to enter text.** | **Click here to enter text.** |
| **B** | **Location: SAT 2** |  | | | | |
|  | * Type: 18W LED tube (daylight) |  | **3** | | **Click here to enter text.** | **Click here to enter text.** |
| * Type: 36W fluorescent tube (daylight) |  | **3** | | **Click here to enter text.** | **Click here to enter text.** |
| * Type: Dimmable ballast for 2x36W fluorescent fitting |  | **2** | | **Click here to enter text.** | **Click here to enter text.** |
| * Type: Dimmable ballast for 1x36W fluorescent fitting |  | **2** | | **Click here to enter text.** | **Click here to enter text.** |
| **C** | **Location: Mortar Room** |  | | | | |
|  | * Type: 18W LED tube (daylight) |  | **10** | | **Click here to enter text.** | **Click here to enter text.** |
| * Type: 9W LED tube (daylight) |  | **2** | | **Click here to enter text.** | **Click here to enter text.** |
| * Type: Replace existing 4x9W LED fitting tube to 18W fluorescent tube comes with modification of wiring |  | **3** | | **Click here to enter text.** | **Click here to enter text.** |
| * Type: Dimmable ballast for 4x18W fluorescent fitting |  | **3** | | **Click here to enter text.** | **Click here to enter text.** |
| * Type: Lighting point using 3x1 C/1.5mm² PVC cable in PVC conduit comes with dimmer switch |  | **1** | | **Click here to enter text.** | **Click here to enter text.** |
| **d** | **Location: Armory Room** |  | | | | |
|  | * Type: 18W LED tube (daylight) |  | **14** | | **Click here to enter text.** | **Click here to enter text.** |
| **E** | **Location: Server Room** |  | | | | |
|  | * Type: 18W LED tube (daylight) |  | **3** | | **Click here to enter text.** | **Click here to enter text.** |
| **F** | **Location:** **Multi-Purpose Store** |  | | | | |
|  | * Type: Replace existing 3x36W fluorescent fitting tubes to 18W LED tubes comes with modification of wiring |  | **3** | | **Click here to enter text.** | **Click here to enter text.** |
| **G** | **Location: Generator Room** |  | | | | |
|  | * Type: Replace existing 1x36W fluorescent fitting tubes to 18W LED tubes comes with modification of wiring |  | **1** | | **Click here to enter text.** | **Click here to enter text.** |
| **H** | **Location: Electrical Room** |  |  | |  |  |
|  | * Type: 18W LED tube (daylight) |  | **2** | | **Click here to enter text.** | **Click here to enter text.** |
| **I** | **Location: Conference Room** |  | | | | |
|  | * Type: 36W Fluorescent tube (daylight) |  | **3** | | **Click here to enter text.** | **Click here to enter text.** |
| * Type: Dimmable ballast for 2x36W fluorescent fitting |  | **1** | | **Click here to enter text.** | **Click here to enter text.** |
| * Type: Dimmable ballast for 1x36W fluorescent fitting |  | **1** | | **Click here to enter text.** | **Click here to enter text.** |
| **J** | **Location: TSC Signage** |  | | | | |
|  | * Type: 18W LED tube (daylight) |  | **2** | | **Click here to enter text.** | **Click here to enter text.** |
| * Erect scaffold to replace defective LED tubes and dismantle |  | **1** | | **Click here to enter text.** | **Click here to enter text.** |
| **H** | **Location: Streetlight** |  | | | | |
|  | * Type: 120W LED streetlight lantern |  | **2** | | **Click here to enter text.** | **Click here to enter text.** |
|  | Note:   * The address is at: BELTS Simulation Training Centre, Penanjong Camp, Tutong. * For any site visit request, kindly email your proposed date & time schedule to [admincorp@belts.com.bn](mailto:admincorp@belts.com.bn) * For any questions or enquiries, kindly email directly to [rfq\_enquiry@belts.com.bn](mailto:rfq_enquiry@belts.com.bn) * Contractors must implement safety measures to protect workers and public during installation/delivery work. * Vendors/contractors must adhere to regulatory SHENA safety rules and regulations. * The vendor participating in this RFQ is required to submit a complete Permit To Work (PTW) documentation in accordance with the checklist provided in Annex B. The PTW documents shall be compiled and submitted as a single combined PDF file. | | | | | |
| **MANDATORY**  Suppliers are to provide with the Packaging Dimension, Measurement & Weight - in Standard measurement in Meter, Feet, Inches, Cm, Mm, Kg, GM | | | | **TOTAL PRICE** | | **Click here to enter text.** |
| Freight Term (EXW, CIF, ETC) | | | | | | **Click here to enter text.** |
| Freight Charges (IF APPLICABLE) | | | | | | **Click here to enter text.** |
| Any other charges please state | | | | | | **Click here to enter text.** |
| **GRAND TOTAL** | | | | | | **Click here to enter text.** |

|  |  |
| --- | --- |
| Currency Code: | **BND** |
| Price Validity  (Minimum 9 Months): | **Click here to enter text.** |
| Payment Terms: | **30 DAYS CREDIT** |
| Warranty: | **Click here to enter text.** |
| Mode of Delivery: | **Click here to enter text.** |
| Delivery Period: | **Click here to enter text.** |
| Country of Manufactured: | **Click here to enter text.** |
| Remarks: | **Click here to enter text.** |